LED recessed luminaire, BASIC series, for 625 mm ceiling module. Flat shape. Aluminium frame, white, powder-coated. Diffuser made from plastic (PMMA), opal, non-yellowing. Power supply, can be switched or dimmed (DALI/TRIAC dimmer), external. Version with CASAMBI® Bluetooth control available.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Impact resistance: IK 03

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 36 W

Photometrical data:

Rated luminous flux: 3.800 lm

Colour temperature: 4000 K

UGR: 21.1

Light source: LED

Physical data:

Length (L): 620 mm

Width (B): 620 mm

Height (H): 10 mm

Manufacturer: RP-Technik GmbH