LED surface-mounted luminaire, HAWK Sport series, IP43, for use in sports halls, gyms and other sports facilities. Impact-resistant in accordance with DIN 18032-3. Housing made from steel plate, powder-coated. Diffuser made from PC, UV-resistant. Power supply, can be switched or dimmed (DALI dimmer), integrated. Version with CASAMBI® Bluetooth control available. DC compatible. NANO protection on request.

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 43

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 18 W

Photometrical data:

Rated luminous flux: 1.650 lm

Colour temperature: 4000 K

UGR: 20.2

Light source: LED

Physical data:

Length (L): 520 mm

Width (B): 355 mm

Height (H): 74 mm

Manufacturer: RP-Technik GmbH