miniControl plus
MC central emergency power supply system without power limitation in accordance with DIN EN 50171:2021 and DGUV Regulation 3 for supplying emergency and escape sign luminaires {{(P:20:56)}} / {{(P:20:55)}} AC/DC {{(P:20:50)}}.
Suitable for emergency lighting systems in accordance with:
• DIN VDE 0100-718:2014-06 (Requirements in special operating areas – Emergency lighting),
• DIN VDE 0100-560:2022-10 (Emergency power supply),
• DIN EN 50172:2024-10 (VDE 0108-100:2024-10) (Emergency lighting systems).
With automatic test device and individual luminaire monitoring, as well as individual status display for each luminaire in the control unit – in conjunction with system-specific electronic ballasts including a monitoring module, without an additional data line.
Rated operating time / maximum connected load:
○ 1 h / max. {{(P:20:130)}}
○ 3 h / max. {{(P:20:131)}}
○ 8 h / max. {{(P:20:132)}}
Recharge time: 12 h
Consists of:
Microprocessor control unit with integrated IO module for reporting operating states and remote triggering of function tests and emergency light blocking.
Charging device with microprocessor-controlled charging for standard-compliant battery charging.
Integrated control cabinet interior lighting.
For accommodating up to a maximum of 6 DCM variable circuit modules, each with 2 circuits, and a maximum of one 1.0A charging module.
{{(P:6:24)}}- {{(P:19:239)}}, with partially sealed electronics and battery compartment for up to 18 OGIV batteries, max. 17 Ah
Dimensions: H={{(P:1:2)}}, W={{(P:1:1)}}, D={{(P:1:8)}}
Protection class: {{(P:19:239)}} {{(P:18:31)}}, {{(P:18:32)}} incl. wall mount
Cable entry: Standard from the top
Exterior finish: Textured powder coating
Color: {{(P:5:23)}}

Brand: RP-Technik GmbH
