Emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 und DIN EN 1838. Emergency luminaire in a sleek Aluminium profile, matt andonized for ceiling mounting with an additional light source to light the Floor below the luminaire. Housing is openable toollessly. Applicable for maintained or non-maintained operation. The toolless change and variable use of these pictograms provide planning security on site. Pluggable set of pictograms (left, right, down, up) is included in the scope of delivery. 

Material: Aluminum
Color: Alu eloxiert
Dimensions: 62 mm x 258 mm x 147 mm

Mounting method: Deckenaufbau
Protection class: 1
Protection rating (IP): IP 40
Impact restistence rate IK: IK 3
Allowed temperature DS: -25 °C to 40 °C °C
Allowed temperature BS: -25 °C to 40 °C °C
Viewing distance: 22m m
Pictogram: Set

Power maintained mode: 4,5 W W
Power non-maintained mode: 0 W W

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

Article number: LMD019

Accessories:
Article number: DSA, cord suspension set 1,5m
Article number: 2PS-EB
Article number: AWM001-SI, Wall bracket, silver convenient for RM, RI, LM, AS, KT, MMD

Brand: RP-Technik GmbH
