Emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 und DIN EN 1838. Emergency luminaire in a sleek Aluminium profile, matt andonized for wall mounting with an additional light source to light the Floor below the luminaire. Housing is openable toollessly. Applicable for maintained or non-maintained operation. The toolless change and variable use of the pictograms provide planning security on site. Pluggable set of pictograms (left, right, down, up) is included in the scope of delivery. 

Material: Aluminum
Color: Alu eloxiert
Dimensions: 62 mm x 614 mm x 334 mm

Mounting method: Wandaufbau
Protection class: 1
Protection rating (IP): IP 40
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -25 °C to 40 °C °C
Allowed temperature BS: -25 °C to 40 °C °C
Viewing distance: 56m m
Pictogram: Einzeln n.A.

Power maintained mode: 5,2 W W
Power non-maintained mode: 0 W W

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

Article number: LSW019

Accessories:

Brand: RP-Technik GmbH
