Emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 und DIN EN 1838. Emergency luminaire in a sleek Aluminium profile, matt andonized for ceiling mounting with an additional light source to light the Floor below the luminaire. Housing is openable toollessly. Applicable for maintained or non-maintained operation. The toolless change and variable use of the pictograms provide planning security on site. 
Switch-mode power supply up to 5W for LED lights Set-up of various output voltages (3.3V/5V/12V/24V) possible. The NT24 power supply can be used in conjunction with a monitoring module for use in the following emergency light system types: my-, micro-, mini-, midi and multiControl. The respective output voltage is set via the switch.
Material: Aluminum
Color: Alu eloxiert
Dimensions: 62 mm x 614 mm x 334 mm

Mounting method: Deckenaufbau
Protection class: 1
Protection rating (IP): IP 40
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -25 °C to 40 °C °C
Allowed temperature BS: -25 °C to 40 °C °C
Viewing distance: 56m m
Pictogram: Einzeln n.A.

Power maintained mode: 5,2 W W
Power non-maintained mode: 0 W W

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

Article number: LSD019

Accessories:
Article number: DSA, cord suspension set 1,5m
Article number: 2PS-EB

Brand: RP-Technik GmbH
