LED safety light in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.  Rechargeable portable spotlight with 3W Power LED and magnetic base, for flexible mounting on metals e.g. control cabinets.  In case of a power failure the emergency light function switches on automatically. The luminaire head can be swivelled backwards by 110° and forwards by 70°.  Includes a flashing and dimming feature for longer burning periods. Wall bracket with charging function, 230V power supply unit (12V vehicle charger optional). 
Material: Polycarbonate
Color: RAL 9005
Dimensions: 104 mm x 130 mm x 300 mm

Mounting method: Wandaufbau
Protection class: 2
Protection rating (IP): IP 54
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: 0 °C to 40 °C °C
Allowed temperature BS: 0 °C to 40 °C °C
Pictogram: Nein

Luminous Flux Emergency Operation: 180 lm lm

Battery: HXACC, HX Battery

Article number: HX

Accessories:
Article number: HXNT12, HX 12V car adapter / charging cable EUP Adaptor
Article number: HXOSD, HX organge glass Orange Signal Diffuser
Article number: HXACC, HX Akkumulator LFP HxBxL 19 x 36,5 x 66,5mm  Li-ion 7.4V / 1600 mAh

Brand: RP-Technik GmbH
