Escape sign luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838  Metal escape sign luminaire for recessed wall mounting, with front frame secured by screws. Suitable for continuous or stand-by operation. Planning reliability due to variable use of pictograms on site. Pictograms according to DIN EN ISO 7010 and DIN ISO 3864 (left, right, bottom, top) included as standard.

Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Material: Metal
Color: RAL 9003
Dimensions: 65 mm x 280 mm x 160 mm

Mounting method: Wandeinbau
Protection class: 1
Protection rating (IP): IP 40
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 22m m
Pictogram: Set

Power maintained mode: 7,5 W W
Power non-maintained mode: 3,6 W W
Luminous Flux Emergency Operation: 150 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: NIMH1208P, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: U6E013WL

Accessories:
Article number: U6BE, U6 concreate housing

Brand: RP-Technik GmbH
