Emergency sign / safety light in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.Cuboid shaped synthetic housing, with it’s discreet look, the luminaire design is concentrating on essentials.

Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: Polycarbonate
Color: RAL 9003
Dimensions: 326 mm x 50 mm x 50 mm

Mounting method: Universal
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 5
Allowed temperature DS: -30 °C to 35 °C °C
Allowed temperature BS: -30 °C to 35 °C °C
Viewing distance: 14m,22m,30m m
Pictogram: Einzeln n.A.

Power maintained mode: 5,9 W W
Power non-maintained mode: 1,1 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: KBDUO029ML

Accessories:
Article number: KBK, KB disc VD 14m incl. pictoset
Article number: KBM, KB disc VD 22m incl. pictoset
Article number: KBG, KB disc VD 30m incl. pictoset
Article number: AWX001, Wall bracket, white convenient for RX, KB, KX, KW, LX, GX, KE
Article number: KBE, KB recessed frame - ABS white  exkl. test button
Article number: BALLPLX-KBE, Ball protection  465x181x31mm incl. fastening Plexiglas clear for KBU recessed
Article number: BALLPLX-KBS, Ball protection 410x322x77mm incl. fastening  Plexiglas clear for KB incl. edge
Article number: BALLPLX-KBU, Ball protection 420x150x77mm outside Plexiglas clear, for KB witout edge
Article number: 2PW-EB, Double - Pendulum white 500mm  pre-wired with 4-wires
Article number: 2DW-EB
Article number: KBBE
Article number: DSA, cord suspension set 1,5m

Brand: RP-Technik GmbH
