General and emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Round, attractively shaped LED general luminaire made of aluminium for wall or ceiling mounting with emergency lighting insert. Emergency lighting is provided by means of an additionally integrated emergency luminaire.  Housing colour choice of anodised aluminium or whiteChoice of light colour 4000 K or 3000 K 

Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Material: Aluminum
Color: Alu eloxiert
Diameter: 395 mm

Mounting method: Universal
Protection class: 1
Protection rating (IP): IP 20
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 30 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 26,4 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 240 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: NIMHHT4820Q, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: QAW023WL-SI

Accessories:

Brand: RP-Technik GmbH
