miniControl XL plus
Central emergency power supply system MC with limited power (LPS) in accordance with EN 50171 and BGV A3 for supplying 230V/216V AC/DC safety and escape sign luminaires. Suitable for emergency lighting systems in accordance with DIN VDE 0100-718, DIN VDE 0100-560, DIN EN 50172, and DIN V VDE V 0108-100.
With automatic test device and individual luminaire monitoring with individual status display for each luminaire in the control unit in conjunction with system-specific electronic ballasts including a monitoring module without an additional data line.
Rated operating time / maximum connected load:
○ 1 h / max. 1500 W
○ 3 h / max. 500 W
○ 8 h / max. 300 W
Recharging time: 12 h
Consists of:
Microprocessor control unit with DB25 Centronics printer interface and integrated IO module for reporting operating states and remote triggering of function tests and emergency light blocking.
Charging unit with microprocessor-controlled charging for standard-compliant battery charging.
For accommodating up to 16 DCM variable circuit modules, each with two circuits, and a maximum of one 1.0 A charging module.
Sheet steel combination cabinet with partially sealed electronics and battery compartment for up to 18 OGIV batteries, max. 17 Ah
Dimensions: H = 1470 mm, W = 571 mm, D = 230 mm
Protection rating: Electronics cabinet IP 20, Protection Class I
Includes wall mounting
Cable entry: Standard from the top
Exterior finish: Textured powder coating
Color: RAL 7035 light gray

Brand: RP-Technik GmbH
