Robust zinc die-cast escape sign luminaire for dynamic escape route control for wall mounting.The Flexway escape sign luminaire provides 10 display options. From these, two operating states can be freely selected via rotary coding switch. The operating states are activated via the potential-free contact, e.g. of a smoke detector or fire alarm system. For the use of a potential-free contact, it offers a power-limited and monitored output voltage.Features:- Mechanically robust and corrosion-resistant- Powder-coated surface- Precise edges and straight lines- No welds or bending edges- 10 display options each controllable via potential-free contact

Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: Zinc die-cast
Color: RAL 9003
Dimensions: 58 mm x 262 mm x 188 mm

Mounting method: Wandaufbau
Protection class: 1
Protection rating (IP): IP 65
Impact restistence rate IK: IK 8
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 20m m
Pictogram: Set

Power maintained mode: 5,4 W W
Power non-maintained mode: 2,8 W W

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: FMWD009ML

Accessories:
Article number: FMWA001, Surface mounting adapter for lateral cable feed  white, plastic for FM
Article number: FMFH, flexible wall mounting for FM

Brand: RP-Technik GmbH
