Emergency sign luminaire in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   Slim synthetic luminaire for universal mounting wall/ceiling as well as wall brackets via the included adapter. With additional downwards light emission. Housing can be opened without the use of tools.  Suitable for continuous mode or stand-by mode. Reliable planning due to a toolfree and variable, on-site use of the pictograms. Set of pictograms (left, right, bottom, top) is included in the scope of delivery. The COOL light is equipped with an external battery housing for installation in the building. The installation of the lamp can be done outdoors or in cold stores.

Material: Polycarbonate
Color: RAL 9003
Dimensions: 70 mm x 260 mm x 155 mm

Mounting method: Deckeneinbau
Protection class: 2
Protection rating (IP): IP 43
Impact restistence rate IK: IK 3
Allowed temperature DS: -25 °C to 40 °C °C
Allowed temperature BS: -25 °C to 40 °C °C
Viewing distance: 22m m
Pictogram: Set

Power maintained mode: 4,5 W W
Power non-maintained mode: 0,35 W W
Luminous Flux Emergency Operation: 150 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: NIMHHT4820Q, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: KDU013-COOL

Accessories:
Article number: DSA, cord suspension set 1,5m
Article number: BALL1, Ball protection (6W) 320x220x120mm  RAL9010, for KD, KM, KS, LM, SD, VM
Article number: 2PW-EB, Double - Pendulum white 500mm  pre-wired with 4-wires
Article number: 2DW-EB
Article number: BALLPLX-KD, Ball protection  380x280x100mm incl. fastening Plexiglas clear for KDU wall

Brand: RP-Technik GmbH
