Four-sided LED escape sign luminaire for ceiling mounting according to DIN EN 60598-1, DIN EN 60598-2-22Cube plastic luminaire with frameless bonnet and concealed mounting tray made of galvanised sheet steel.  Suitable for continuous or stand-by operation. Planning reliability due to logically printed pictograms according to DIN EN ISO 7010 and DIN ISO 3864 (left, right, top) as standard.

Material: Metal
Color: RAL 9003
Dimensions: 237 mm x 237 mm x 237 mm

Mounting method: Wandaufbau
Protection class: 1
Protection rating (IP): IP 20
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -25 °C to 40 °C °C
Allowed temperature BS: -25 °C to 40 °C °C
Viewing distance: 46m m
Pictogram: Set

Power maintained mode: 4,5 W W
Power non-maintained mode: 0 W W
Luminous Flux Emergency Operation: 250 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

Article number: WGW019

Accessories:
Article number: WKO, Set out of 4 x chain eyelet  for cube luminaires

Brand: RP-Technik GmbH
