LED exterior façade luminaire, Tondo series. Housing made from die-cast aluminium, dark grey or white, powder-coated, IP54. Diffuser made from plastic (PC), opal, UV-stabilised. Operating unit installed (can be switched). Version with CASAMBI® Bluetooth control available.

Dimensions:
Height: 80 mm
Depth:  mm
Diameter: 280 mm

Packaging dimensions:
Width: 330 mm
Height: 100 mm
Depth: 330 mm

Housing material:

Certification:
Protection type (IP): wert.IngressProtection.IP 54

Electrical connection:
Power maintained: 13 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 985 lm
Color temperature: 3000 K
UGR: 24.2

Temperatures:

Mounting:

Color:

Brand: RP-Technik GmbH
