LED recessed downlights, Cantone series. Four different covers in white, chrome, chrome matt and brushed metal, available in a round/square version. Operating unit can be dimmed (TRIAC/DALI dimmer), external. Version with CASAMBI® Bluetooth control available.

Dimensions:
Width: 92 mm
Height: 50 mm
Depth: 92 mm

Packaging dimensions:
Width: 100 mm
Height: 75 mm
Depth: 130 mm

Cutout Dimensions:
Diameter: 68 mm

Color:

Housing material:

Certification:
Protection type (IP): IP 20

Storage temperature range:

Electrical connection:
Power maintained: 8.1 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:
DC suitability: wert.DCSuitable.Ja
EEK: wert.EEK.B

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 450 lm
Color temperature: 2700 K

Temperatures:

Mounting:

Brand: RP-Technik GmbH
