LED recessed luminaire, frame panel, EDGE series, for 625 mm ceiling module. Flat shape. Aluminium frame, white, powder-coated. Diffuser made from plastic (PMMA), opal, non-yellowing. Power supply, can be switched or dimmed (DALI/TRIAC dimmer), external. Version with CASAMBI® Bluetooth control, RGBW and tunable white available.

Dimensions:
Width: 615 mm
Height: 15 mm
Depth: 615 mm

Packaging dimensions:
Width: 635 mm
Height: 30 mm
Depth: 640 mm

Cutout Dimensions:
Width: 0 mm
Depth: 0 mm

Color:

Housing material:

Certification:
Protection type (IP): IP 20

Electrical connection:
Power maintained: 40 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 0 lm
Color temperature:  K

Temperatures:

Mounting:

label.zuordnungsspeicher.gruppe.Casambi-Products:
Max. transmission power: +4 dBm

Brand: RP-Technik GmbH
