Combined LED general and emergency luminaire for the illumination of escape and rescue routes according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838. The robust LED wall and ceiling luminaire made of glass-fibre reinforced polyester for damp locations is suitable for illuminating storage areas, multi-storey car parks, etc. In mains operation, the luminaire has an output of up to 7,000 lm. Easy quick mounting by means of metal mounting bracket.

Material: Polycarbonate
Color: RAL 7035
Dimensions: 1560 mm x 82 mm x 97 mm

Mounting method: Universal
Protection class: 1
Protection rating (IP): IP 65
Impact restistence rate IK: IK 8
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 54 W W
Luminous Flux Emergency Operation: 6800 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

Article number: LFD15009-NW

Accessories:

Brand: RP-Technik GmbH
