LED recessed luminaire, BASIC series, for 625 mm ceiling module. Flat shape. Aluminium frame, white, powder-coated. Diffuser made from plastic (PMMA), opal, non-yellowing. Power supply, Switchable external. Version with CASAMBI® Bluetooth control available.

Dimensions:
Width: 620 mm
Height: 10 mm
Depth: 620 mm

Packaging dimensions:
Width: 650 mm
Height: 45 mm
Depth: 690 mm

Cutout Dimensions:

Color:

Housing material:

Certification:
Protection type (IP): IP 20
Shock resistance level (IK): wert.IKclass.IK 3

Electrical connection:
Power maintained: 36 W
Input voltage AC: 220-240V / 50-60Hz V

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 3800 lm
Color temperature: 4000 K
UGR: 21.1

Temperatures:

power supply:

Brand: RP-Technik GmbH
