LED recessed and surface-mounted downlight, RAVIO series. IP20 (for the surface-mounted version). Housing made from plastic (PC) and passive aluminium cooler. Diffuser made from plastic, opal. Operating unit can be switched or dimmed (DALI dimmer), external (integrated in the surface-mounted version). Version with Casambi Bluetooth control available. DC compatibility on request.

Dimensions:
Height: 80 mm
Diameter: 172 mm

Packaging dimensions:
Width: 190 mm
Height: 145 mm
Depth: 190 mm

Cutout Dimensions:
Diameter: 160 mm

Color:

Housing material:

Certification:
Protection type (IP): wert.IngressProtection.IP 44

Electrical connection:
Power maintained: 23 W
Input voltage AC: 220-240V / 50-60Hz V

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 2450 lm
Color temperature: 4000 K

Temperatures:

Mounting:

power supply:

Brand: RP-Technik GmbH
