LED ceiling- and wall-mounted luminaire, RONDO series, with direct/indirect beam, as the basic lighting for rooms in a commercial environment and at home. Housing made from aluminium, white, powder-coated. Diffuser made from plastic (PMMA), opal, UV-stabilised. Operating unit can be switched or dimmed (DALI dimmer), integrated. Version with CASAMBI® Bluetooth control available. DC compatible.

Dimensions:
Height: 62 mm
Diameter: 600 mm

Packaging dimensions:
Width: 610 mm
Height: 100 mm
Depth: 610 mm

Color:

Housing material:

Certification:
Protection type (IP): wert.IngressProtection.IP 40

Electrical connection:
Power maintained: 39 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:
DC suitability: wert.DCSuitable.Ja

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 5450 lm
Color temperature: 4000 K
UGR: 21

Temperatures:

Mounting:

Brand: RP-Technik GmbH
