LED track luminaires, Track series, with multi-adapter for 3-phase busbars, 230V. Housing made from die-cast aluminium, white or anthracite, powder-coated. Can be rotated 350° horizontally and swivelled 90° vertically. Interchangeable PC lenses, non-yellowing, for various beam angles (20° - 60°). Operating unit can be switched or dimmed (DALI dimmer), installed.

Dimensions:
Width: 150 mm
Height: 85 mm
Depth: 184 mm

Packaging dimensions:
Width: 140 mm
Height: 110 mm
Depth: 208 mm

Color:

Housing material:

Certification:
Protection type (IP): IP 20

Electrical connection:
Power maintained: 15 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 1600 lm
Color temperature: 4000 K
UGR: 16.7

Temperatures:

Brand: RP-Technik GmbH
