LED moisture-proof luminaire, SWIM series, IP69, IK08. The luminaire may be immersed to a depth of 10 m. Housing and side sections made from polycarbonate(PC), grey (UV- and chlorine-resistant). Opal diffuser made from PC, UV- and chlorine-resistant. Symmetric light distribution and homogeneous illumination. Feed-through wiring present. Power supply, can be switched or dimmed (DALI dimmer), integrated. NANO protection on request. Area of application: car washes, chemical industry, swimming pools etc.

Dimensions:
Width: 70 mm
Height: 70 mm
Depth: 780 mm

Packaging dimensions:
Width:  mm
Height:  mm
Depth:  mm

Housing material:

Certification:
Protection type (IP): wert.IngressProtection.IP 66
Shock resistance level (IK): wert.IKclass.IK 10

Electrical connection:
Power maintained: 17 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 1900 lm
Color temperature: 4000 K
UGR: 25.5

Temperatures:

Mounting:

Brand: RP-Technik GmbH
