LED ceiling- and wall-mounted luminaire, MAVS. Housing made from aluminium, white, powder-coated. Diffuser made from plastic (PMMA), opal, UV-stabilised. Operating unit can be switched or dimmed (DALI dimmer), integrated. Version withCASAMBI® Bluetooth control available. DC compatible.

Dimensions:
Width: 79 mm
Height: 79 mm
Depth: 1425 mm

Packaging dimensions:
Width: 119 mm
Height: 74 mm
Depth: 1600 mm

Cutout Dimensions:

Color:

Housing material:

Certification:
Protection type (IP): wert.IngressProtection.IP 40

Electrical connection:
Power maintained: 44 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:
DC suitability: wert.DCSuitable.Ja

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 4600 lm
Color temperature: 4000 K
UGR: 26.2

Temperatures:

Mounting:

Brand: RP-Technik GmbH
