LED ceiling- and wall-mounted luminaire, MAVS. Housing made from aluminium, white, powder-coated. Diffuser made from plastic (PMMA), opal, UV-stabilised. Operating unit can be switched or dimmed (DALI dimmer), integrated. Version withCASAMBI® Bluetooth control available. DC compatible.

Dimensions:
Width: 59 mm
Height: 79 mm
Depth: 570 mm

Packaging dimensions:
Width: 118 mm
Height: 75 mm
Depth: 690 mm

Color:

Housing material:

Certification:
Protection type (IP): wert.IngressProtection.IP 40

Electrical connection:
Power maintained: 17 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:
DC suitability: wert.DCSuitable.Ja

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 1700 lm
Color temperature: 3000 K
UGR: 26.2

Temperatures:

Mounting:

Brand: RP-Technik GmbH
