LED ceiling- and wall-mounted luminaire, ZORRO. Housing made from steel plate, white, powder-coated. Diffuser made from plastic (PC), opal, UV-stabilised. Operating unit can be switched or dimmed (DALI dimmer), integrated. Version with CASAMBI® Bluetooth control available. DC compatible. NANO protection on request.

Dimensions:
Width: 165 mm
Height: 63 mm
Depth: 600 mm

Packaging dimensions:
Width: 166 mm
Height: 57 mm
Depth: 704 mm

Color:

Housing material:

Certification:
Protection type (IP): wert.IngressProtection.IP 40

Electrical connection:
Power maintained: 19 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 2200 lm
Color temperature: 4000 K
UGR: 26

Temperatures:

Mounting:

Brand: RP-Technik GmbH
