LED moisture-proof luminaire, LUKA series, IP66. Resistant to ammonia and oil. Housing made from steel plate. Diffuser made from safety glass. Feed-through wiring present. Power supply, can be switched or dimmed (DALI dimmer), integrated. DC compatibility and NANO protection on request. Suitable for use in the food industry. Area of application: car washes, chemical industry, kitchens etc.

Dimensions:
Width: 192 mm
Height: 90 mm
Depth: 1305 mm

Packaging dimensions:
Width: 250 mm
Height: 150 mm
Depth: 1360 mm

Color:

Housing material:

Certification:
Protection type (IP): wert.IngressProtection.IP 66

Electrical connection:
Power maintained: 35 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:
DC suitability: wert.DCSuitable.Ja

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 3950 lm
Color temperature: 4000 K
UGR: 21.5

Temperatures:

Mounting:

Brand: RP-Technik GmbH
