LED recessed and surface-mounted downlight, DOALA series, for ceiling recesses of 65 mm to 205 mm. Housing made from aluminium, white, powder-coated. Diffuser made from PS, opal. Operating unit integrated (can be switched). Three-stage adjustment of colour temperature (3000K, 4000K, 5700K) using DIP switch. Version with CASAMBI Bluetooth control available.

Cutout Dimensions:
Depth: 0 mm

Color:

Housing material:

Certification:
Protection type (IP): IP 20

Electrical connection:
Power maintained: 17 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:
DC suitability: wert.DCSuitable.Nein

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 1650 lm
Color temperature: 3000/4000/6000 K
UGR: 27.5

Temperatures:

Mounting:

Dimensions:
Width: 235 mm
Height: 15 mm
Depth: 235 mm

Packaging dimensions:

Brand: RP-Technik GmbH
