General and emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Round, attractively shaped LED general luminaire made of aluminium for wall or ceiling mounting with emergency lighting insert. Emergency lighting is provided by means of an additionally integrated emergency luminaire.  Housing colour choice of anodised aluminium or whiteChoice of light colour 4000 K or 3000 K 

Monitoring: 
Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:
· Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
· Automatic function test (weekly)
· Automatic continuous function test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
· Idling and short-circuit shutdown of inverter
Material: Aluminum
Color: Alu eloxiert
Diameter: 395 mm

Mounting method: Universal
Protection class: 1
Protection rating (IP): IP 20
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 30 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 26,4 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 110 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: NIMHHT4820Q, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: QAW028SC-SI-BM

Accessories:

Brand: RP-Technik GmbH
