General and emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Round, attractively shaped LED general luminaire made of aluminium for wall or ceiling mounting with emergency lighting insert. Emergency lighting is provided by means of an additionally integrated emergency luminaire.  Housing colour choice of anodised aluminium or whiteChoice of light colour 4000 K or 3000 K 

Monitoring: 
With integrated monitoring module for operation on a monitoring device of the Wireless Basic type.
· Time-saving configuration and commissioning as well as monitoring via Bluetooth using an Android app
· Operation in offline mode or optionally via LIGHTLINX® with versatile cloud functions
· Version with automatic test system according to DIN EN 62034 type S incl. SelfControl test button
· Test results with fault analysis (illuminant, charging and battery circuit) as well as status displays (operation, function test, duration test) via 3 coloured LEDs
· Manual or automatic function test (test start time freely selectable in the WirelessBasic app)
· Configurable duration test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart lockout
· No-load and short-circuit shutdown of the inverter
Material: Aluminum
Color: Alu eloxiert
Diameter: 395 mm

Mounting method: Universal
Protection class: 1
Protection rating (IP): IP 20
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 30 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 26,4 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 110 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: NIMHHT4820Q, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: QAW028WB-BM

Accessories:

Brand: RP-Technik GmbH
