Emergency sign / safety light in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   Slim, convex, synthetic luminaire for wall mounting. Emergency sign luminaire with pluggable, solvent-free, internal set of pictograms (left, right, bottom, top) included in the scope of delivery. Also usable as safety light without applying the pictograms, as it includes a clear-transparent cover. Evenly distributed illumination, due to the alligned and chromed reflector. Suitable for continuous mode or stand-by mode. 

Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: Polycarbonate
Color: RAL 9003
Dimensions: 90 mm x 340 mm x 170 mm

Mounting method: Deckenaufbau
Protection class: 1
Protection rating (IP): IP 64
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -20 °C to 40 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Viewing distance: 30m m
Pictogram: Set

Power maintained mode: 5,2 W W
Power non-maintained mode: 1,1 W W
Luminous Flux Emergency Operation: 300 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: KCD019ML-IP64

Accessories:
Article number: WKL, surcharge 2 x chain eyelet  for luminaires

Brand: RP-Technik GmbH
