WirelessProfessional system in accordance with DIN EN 62034, VDE 0711-400 and DIN EN 60598-2-22 with approval in the 868 MHz band in accordance with ETSI EN 300 220
Touch netbook with installed WirelessProfessional software and USB coordinator. For monitoring and controlling the WirelessProfessional single-battery lights.
Automatic test system in accordance with EN 62034 type ER
The status of the system and the status of each device are symbolically displayed in the software for visual perception.
System features:
- Monitoring of self-contained luminaires (WL) wirelessly via radio 868 MHz, without additional data line
- Monitoring of up to 250 wireless devices, e.g. lights or IO box
- Expandable in increments of 250 up to a total of 1,000 devices per control centre
- Range between wireless devices guaranteed at 30 m inside buildings
- Stable, self-organising AdHoc network
- Each wireless device is also a repeater
- Multilingual user interface of the software
- User interface with different user levels through rights management (e.g. building technician, installer, etc.)
- Energy-saving function for idle times
- Status and error messages can be conveniently sent by e-mail
- Remote access via the Internet possible
- Luminaires can be switched in groups or individually via the central unit by radio
- Visualisation of luminaire positions and statuses on a building plan or several building plans
- Storage of all system and test data
- Option to call up and print out the test logbook
- Integrated level meter for displaying the radio field strength of radio subscribers
- Automatic function test with daily/weekly interval and freely selectable test times
- Automatic annual operating time test (test duration in individual cases up to 8 hours) possible
- Possibility of manually triggering function tests or operating duration tests
- Safety function guaranteed even if the communication interface fails
Automatic registration of the lights to the central unit with transmission of
1. luminaire type with image information
2. battery type
3. rated operating time
4. switching mode (permanent switching/standby switching)
Scope of delivery:
- TouchNotebook
- WirelessProfessional software
- USB coordinator with fault signalling contact
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