Escape Route Luminaire with ERT LED for Trilux E-Line Trunking System (Profile 07650, 7-core)This escape route luminaire is specifically designed for the Trilux E-Line trunking system with a 7-core profile (07650). The integrated, innovative lens holder with quick-mounting functionality allows for easy and flexible use of different lens types – perfectly tailored to the specific application.The scope of delivery includes both a lens for area lighting and one for corridor lighting.

Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: Metal
Color: RAL 9003
Dimensions: 368 mm x 62 mm x 40.7 mm

Mounting method: Schienensysteme
Protection class: 1
Protection rating (IP): IP 20
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 5,4 W W
Power non-maintained mode: 1,1 W W
Luminous Flux Emergency Operation: 470 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: LBLT039ML

Accessories:
Article number: LSYS-H4, 4x h-lenses for luminaires with lens  system
Article number: LSYS-S4, 4x Spotlens for luminares with lens system.  Suitable for ceilings up to 12m
Article number: LSYS-B4, 4x Beam lens for lights with a lens system, for  example for lighting first aid or fire alarm  systems

Brand: RP-Technik GmbH
