LED emergency luminaire in accordance with DIN EN 60598-1, DIN EN 60598-2-22, and DIN EN 1838.Round LED emergency luminaire made of die-cast zinc for ceiling installation. The high-performance LED ensures optimal light distribution and illumination of escape and rescue routes, even with high ceilings.Easy installation is achieved with spring-loaded mounting.

Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: Zinc die-cast
Color: RAL 9003
Diameter: 88 mm

Mounting method: Deckeneinbau
Protection class: 2
Protection rating (IP): IP 40
Impact restistence rate IK: IK 8
Allowed temperature DS: -10 °C to 40 °C °C
Allowed temperature BS: -10 °C to 50 °C °C
Pictogram: Nein

Power maintained mode: 9,6 W W
Power non-maintained mode: 1,1 W W
Luminous Flux Emergency Operation: 1100 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: DDEF039ML

Accessories:
Article number: BALLPLX-ILE, Ball protection  190x190x62mm incl. fastening Plexiglas clear for ILE

Brand: RP-Technik GmbH
