
Monitoring: 
With integrated monitoring module, for operation on a 24V power supply system. Automatic test system in accordance with DIN EN 62034 type ER, in conjunction with a CoreCompact system. Functions must be complied with:
· Integrated individual luminaire monitoring
· Automatic addressing via configuration wizard
· Luminaires can be individually programmed and dimmed with RP's central power supply system
· Luminaire update via the system
Material: Polycarbonate
Color: RAL 9003
Dimensions: 300 mm x 300 mm x 110 mm

Mounting method: Wandaufbau
Protection class: 3
Protection rating (IP): IP 65
Impact restistence rate IK: IK 4
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 30m m
Pictogram: Einzeln n.A.

Power maintained mode: 5,1 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 24 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: WFXW519CC

Accessories:

Brand: RP-Technik GmbH
