Emergency sign / safety light in accordance to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   Slim, convex, synthetic luminaire for wall mounting. Emergency sign luminaire with pluggable, solvent-free, internal set of pictograms (left, right, bottom, top) included in the scope of delivery. Also usable as safety light without applying the pictograms, as it includes a clear-transparent cover. Evenly distributed illumination, due to the alligned and chromed reflector. Suitable for continuous mode or stand-by mode. 

Monitoring: 
With integrated monitoring module, for operation on a 24V power supply system. Automatic test system in accordance with DIN EN 62034 type ER, in conjunction with a CoreCompact system. Functions must be complied with:
· Integrated individual luminaire monitoring
· Automatic addressing via configuration wizard
· Luminaires can be individually programmed and dimmed with RP's central power supply system
· Luminaire update via the system
Material: Polycarbonate
Color: RAL 9003
Dimensions: 90 mm x 340 mm x 170 mm

Mounting method: Deckenaufbau
Protection class: 3
Protection rating (IP): IP 40
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 30m m
Pictogram: Set

Power maintained mode: 4,2 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 335 lm lm

Input voltage AC: 24 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: KCD519CC

Accessories:
Article number: KCAWW, KC plastic wall bracket white Flag mounting
Article number: DSA, cord suspension set 1,5m
Article number: 2PW-EB, Double - Pendulum white 500mm  pre-wired with 4-wires
Article number: WKL, surcharge 2 x chain eyelet  for luminaires

Brand: RP-Technik GmbH
