LED diffuser luminaire, VASCA series, IP65, IK08. Housing made from polycarbonate. Prismatic diffuser made from PC, UV-resistant. Diffuser is fastened with stainless steel clips. LED boards can be interchanged individually. switchable, Feed-through wiring present. Version with Casambi Bluetooth control available. DC compatible.

Dimensions:
Width: 97 mm
Height: 82 mm
Depth: 1560 mm

Packaging dimensions:
Width: 100 mm
Height: 90 mm
Depth: 1585 mm

Housing material:

Certification:
Protection type (IP): wert.IngressProtection.IP 65
Shock resistance level (IK): wert.IKclass.IK 8

Electrical connection:
Power maintained: 36 W
Input voltage AC: 220-240V / 50-60Hz V

power supply:
DC suitability: wert.DCSuitable.Ja

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 4500 lm
Color temperature: 4000 K
UGR: 24

Temperatures:

Mounting:

Brand: RP-Technik GmbH
