LED spotlight, SOLID series. Die-cast aluminium housing, suitable for outdoor use, colour: black, powder-coated. Cover made of tempered glass. Robust housing with IP 66 and high impact resistance IK08. Powerful LED technology with over 140lm/W for effective illumination of large areas. Switchable control gear, built-in. Extremely flexible use thanks to flat design and adjustable angle of inclination. Connection via open cable end.

Dimensions:
Width: 187 mm
Height: 37 mm
Depth: 247 mm

Color:

Housing material:

Certification:
Protection type (IP): wert.IngressProtection.IP 66
Shock resistance level (IK): wert.IKclass.IK 8

Electrical connection:
Input voltage AC: 220-240V / 50-60Hz V
Nominal output: 50 W

power supply:
DC suitability: wert.DCSuitable.Ja

Light data:
Light source: wert.LightSource.LED
Rated luminous flux: 7000 lm
Color temperature: 4000 K

Temperatures:

label.zuordnungsspeicher.gruppe.Casambi-Products:
Input voltage DC: 216 V

Mounting:

Brand: RP-Technik GmbH
