
Monitoring: 
Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:
· Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
· Automatic function test (weekly)
· Automatic continuous function test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
· Idling and short-circuit shutdown of inverter
Material: Polycarbonate
Color: RAL 9003
Dimensions: 300 mm x 300 mm x 110 mm

Mounting method: Wandaufbau
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 4
Allowed temperature DS: 0 °C to 35 °C °C
Allowed temperature BS: 0 °C to 35 °C °C
Viewing distance: 30m m
Pictogram: Einzeln n.A.

Power maintained mode: 4,6 W W
Power non-maintained mode: 0,35 W W
Luminous Flux Emergency Operation: 220 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: NIMH9620Q, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: WFXW018SC

Accessories:
Article number: NIMHHT4820Q, battery pack 4,8V/2,0Ah NimH, 300mm wire (LPU,LEM)

Brand: RP-Technik GmbH
