
Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: Polycarbonate
Color: RAL 9003
Dimensions: 300 mm x 300 mm x 110 mm

Mounting method: Wandaufbau
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 4
Allowed temperature DS: -20 °C to 40 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Viewing distance: 30m m
Pictogram: Einzeln n.A.

Power maintained mode: 5,2 W W
Power non-maintained mode: 1,1 W W
Luminous Flux Emergency Operation: 520 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: WFXW019ML

Accessories:

Brand: RP-Technik GmbH
