Emergency sign luminaire in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Plastic LED emergency sign luminaire with convex cover for wall mounting. Suitable for continuous or standby operation. Levelling screws are integrated to compensate for uneven surfaces and facilitate installation. Planning reliability is ensured by the tool-free, variable use of pictograms on site. The pictograms are internal and are inserted without the use of solvents. The pictogram set (MTL, MTR and 2x straight arrow) is included as standard.

Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Material: Polycarbonate
Color: RAL 9003
Dimensions: 65 mm x 236 mm x 136 mm

Mounting method: Wandaufbau
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 6
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 20m m
Pictogram: Set

Power maintained mode: 2,9 W W
Power non-maintained mode: 0,8 W W

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFPN3216.01-SET

Article number: PMW408WL

Accessories:
Article number: PME, Recessed frame ABS white for PMD and PMW  luminaires
Article number: LFP3216-SET-2AKKU

Brand: RP-Technik GmbH
