
Monitoring: 
Integrated monitoring module for operation with a DALI 2 type monitoring device
· Version with automatic test system according to DIN EN 62034; the type depends on the control unit.
· Automatic test results with fault analysis and status display (operation, function test, endurance test) centrally and at the luminaire via three LEDs.
· Manual or automatic function test configurable by group (test start time freely selectable in the DALI software).
· Configurable endurance test (every 12 months).
· Automatic charging monitoring.
· Deep discharge protection with restart lockout.
Material: Zinc die-cast
Color: RAL 9003
Diameter: 57 mm

Mounting method: Deckenaufbau
Protection class: 3
Protection rating (IP): IP 40
Impact restistence rate IK: IK 6
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 1,5 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 140 lm lm

Input voltage AC: 24 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: IADL529CC

Accessories:

Brand: RP-Technik GmbH
