General and emergency lighting in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Elegant, round LED general light fitting made of aluminium for wall or ceiling mounting with emergency light insert.  Choice of aluminium anodised or white housing colourChoice of 4000 K or 3000 K light colour

Monitoring: 
Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:
· Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
· Automatic function test (weekly)
· Automatic continuous function test (every 12 months)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
· Idling and short-circuit shutdown of inverter
Material: Aluminum
Color: RAL 9003
Diameter: 395 mm

Mounting method: Universal
Protection class: 1
Protection rating (IP): IP 20
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 28 W W
Power non-maintained mode: 2 W W
Luminous Flux Emergency Operation: 360 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: LFP3245.WRLED

Article number: QAW403SC-SI

Accessories:

Brand: RP-Technik GmbH
