General and emergency lighting in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Elegant, round LED general light fitting made of aluminium for wall or ceiling mounting with emergency light insert. Emergency lighting is provided by an additional integrated emergency light.  Choice of aluminium anodised or white housing colourChoice of 4000K light colour with luminous flux in mains operation 2300 lm or 3000K

Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Material: Aluminum
Color: Alu eloxiert
Diameter: 395 mm

Mounting method: Universal
Protection class: 1
Protection rating (IP): IP 20
Impact restistence rate IK: IK ≥ 3
Allowed temperature DS: -5 °C to 30 °C °C
Allowed temperature BS: -5 °C to 35 °C °C
Pictogram: Nein

Power maintained mode: 26,4 W W
Power non-maintained mode: 0,4 W W
Luminous Flux Emergency Operation: 125 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFPN3233.01, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: QAW428WL-SI

Accessories:

Brand: RP-Technik GmbH
