Safety light in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838Plastic LED emergency light with convex moulded cover for ceiling or wall mounting. Suitable for permanent or standby switching. Levelling screws are integrated to make installation easier and compensate for uneven surfaces.The innovative integrated lens holder with quick-mounting device enables the flexible use of different lens types. The most versatile application in this luminaire is the corridor lens, which is already fitted. If necessary, they can be easily replaced with lenses with the desired beam characteristics. This flexibility makes it easy to adapt to the respective installation situation.

Monitoring: 
With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:
· Integrated individual luminaire monitoring
· Integrated luminaire manager function
· Individual switchability in conjunction with RP ELS - central power supply system
Material: Polycarbonate
Color: RAL 9003
Dimensions: 65 mm x 236 mm x 136 mm

Mounting method: Universal
Protection class: 2
Protection rating (IP): IP 65
Impact restistence rate IK: IK 6
Allowed temperature DS: -20 °C to 40 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Pictogram: Nein

Power maintained mode: 9,7 W W
Power non-maintained mode: 1,1 W W
Luminous Flux Emergency Operation: 1050 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: 

Article number: PMW039ML

Accessories:
Article number: PME, Recessed frame ABS white for PMD and PMW  luminaires
Article number: LSYS-B4, 4x Beam lens for lights with a lens system, for  example for lighting first aid or fire alarm  systems
Article number: LSYS-F4, 4x corridor lenses for luminaires with lens  system
Article number: LSYS-H4, 4x h-lenses for luminaires with lens  system
Article number: LSYS-R4, 4x  round lenses for luminaires with lens  system
Article number: LSYS-S4, 4x Spotlens for luminares with lens system.  Suitable for ceilings up to 12m
Article number: LSYS-WF4, 4x wall corridor lenses for luminaires with lens  system

Brand: RP-Technik GmbH
