Frameless and flush-mounted LED escape sign luminaire for wall installation. A luminaire that is perfectly integrated into the wall, with no frame, screws or protruding parts influencing the design of the surroundings.A clever levelling system is already integrated and makes it easy to align the luminaire exactly to the level of the wall.The pictogram set is inserted on the inside and fixed without solvents.

Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Color: Transparent
Dimensions: 100 mm x 212 mm x 110 mm

Mounting method: Wandeinbau
Protection class: 1
Protection rating (IP): IP 40
Impact restistence rate IK: IK 7
Allowed temperature DS: 0 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 20m m
Pictogram: Set

Power maintained mode: 2,2 W W
Power non-maintained mode: 0,8 W W
Luminous Flux Emergency Operation: 80 lm lm

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFPN3212.01-SET

Article number: UEMR413WL

Accessories:

Brand: RP-Technik GmbH
