Frameless and flush-mounted LED escape sign luminaire for wall installation. A luminaire that is perfectly integrated into the wall, with no frame, screws or protruding parts influencing the design of the surroundings.A clever levelling system is already integrated and makes it easy to align the luminaire exactly to the level of the wall.The pictogram set is inserted on the inside and fixed without solvents.
Monitoring: 
With integrated monitoring module, for operation on a 24V power supply system. Automatic test system in accordance with DIN EN 62034 type ER, in conjunction with a CoreCompact system. Functions must be complied with:
· Integrated individual luminaire monitoring
· Automatic addressing via configuration wizard
· Luminaires can be individually programmed and dimmed with RP's central power supply system
· Luminaire update via the system
Color: Transparent
Dimensions: 100 mm x 212 mm x 110 mm

Mounting method: Wandeinbau
Protection class: 1
Protection rating (IP): IP 40
Impact restistence rate IK: IK 7
Allowed temperature DS: -25 °C to 40 °C °C
Allowed temperature BS: -25 °C to 40 °C °C
Viewing distance: 20m m
Pictogram: Set

Article number: UEMR519CC

Accessories:

Brand: RP-Technik GmbH
