Frameless and flush-mounted LED escape sign luminaire for wall installation. A luminaire that is perfectly integrated into the wall, with no frame, screws or protruding parts influencing the design of the surroundings.A clever levelling system is already integrated and makes it easy to align the luminaire exactly to the level of the wall.The pictogram set is inserted on the inside and fixed without solvents.
Switch-mode power supply up to 5W for LED lights Set-up of various output voltages (3.3V/5V/12V/24V) possible. The NT24 power supply can be used in conjunction with a monitoring module for use in the following emergency light system types: my-, micro-, mini-, midi and multiControl. The respective output voltage is set via the switch.
Color: Transparent
Dimensions: 100 mm x 212 mm x 110 mm

Mounting method: Wandeinbau
Protection class: 1
Protection rating (IP): IP 40
Impact restistence rate IK: IK 7
Allowed temperature DS: -20 °C to 40 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Viewing distance: 20m m
Pictogram: Set

Power maintained mode: 1,7 W W
Power non-maintained mode: 0,3 W W
Luminous Flux Emergency Operation: 80 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

Article number: UEMR019

Accessories:
Article number: UEMR-BWE, Recessed housing for concrete and masonry,  designed to accommodate the frameless,  flush-mounted UEMR LED emergency exit sign

Brand: RP-Technik GmbH
