Frameless and flush-mounted LED escape sign luminaire for wall installation. A luminaire that is perfectly integrated into the wall, with no frame, screws or protruding parts influencing the design of the surroundings.A clever levelling system is already integrated and makes it easy to align the luminaire exactly to the level of the wall.The pictogram set is inserted on the inside and fixed without solvents.

Color: Transparent
Dimensions: 100 mm x 212 mm x 110 mm

Mounting method: Wandeinbau
Protection class: 1
Protection rating (IP): IP 40
Impact restistence rate IK: IK 7
Allowed temperature DS: -20 °C to 40 °C °C
Allowed temperature BS: -20 °C to 40 °C °C
Viewing distance: 20m m
Pictogram: Set

Power maintained mode: 1,7 W W
Power non-maintained mode: 0,3 W W
Luminous Flux Emergency Operation: 80 lm lm

Input voltage AC: 230 V V
Connection terminals: 1.5 mm² mm

Battery: 

Article number: UEMR019

Accessories:

Brand: RP-Technik GmbH
