LED escape sign luminaire in accordance with DIN EN 60598-1, DIN EN 60598-2-22, DIN EN 7010 and DIN EN 1838Plastic disc escape sign luminaire for surface mounting on walls and for marking escape and rescue routes. Levelling screws are integrated to facilitate installation and compensate for uneven surfaces. Planning reliability is ensured by the tool-free, variable use of the pictograms on site. The pictograms are inserted solvent-free. The pictogram set (top, bottom, right and left arrows) is included as standard.

Monitoring: 
With integrated monitoring module for operating on a Wireless Professional central monitoring system.
· Charge monitoring indicator on the luminaire
· Manual or automatic function test (free choice of test start time in the WirelessControl software)
· Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
· Automatic charge monitoring
· Deep discharge protection with restart inhibit
Material: Polycarbonate
Color: RAL 9003
Dimensions: 56.1 mm x 417.5 mm x 245.5 mm

Mounting method: Wandaufbau
Protection class: 2
Protection rating (IP): IP 40
Impact restistence rate IK: IK 5
Allowed temperature DS: -5 °C to 40 °C °C
Allowed temperature BS: -5 °C to 40 °C °C
Viewing distance: 40m m
Pictogram: Einzeln n.A.

Power maintained mode: 3,8 W W
Power non-maintained mode: 0,8 W W

Input voltage AC: 230 V V
Connection terminals: 2.5 mm² mm

Battery: LFPN3212.01-SET

Article number: GABW403WL

Accessories:

Brand: RP-Technik GmbH
